DrivHIGH Extremely Savage v1.04 RC1 for Savage2000 Chipset.
Contact Information: obsidianknife@netzero.net

This documents includes the following topics:

Enabling & Disabling Oversampling(FSAA), Installing DrivHIGH Drivers,
and Includes Known Issues, Known Bugs, Known Limitations.


How To Install:
---------------
1. Right-click on an open area of the desktop.
2. Left-click Properties
3. the Display Properties menu should appear, hit the Tab labelled Settings
4. On the bottom hit the bottom that says Advanced...
5. Click on the Adapter Tab
6. Click Change
7. The Update Wizard will appear, click next.
8. Select "Display a list of drivers in a specific location,....
9. click next.
10. Click have Disk.
11. Direct Windows to the DrivHIGH Drivers(default extract location
    is c:\DrivHIGH\ESv001\*.*)
12. Selection the correct adapter, W95 for Windows 95 and W98 for Windows 98
13. Hit Next
14. Hit Next
15. Setup should copy the files.(IMPORTANT!: If when copying files
    you are asked would you like to keep the newer version selection NO!, If you do 
    not select NO you will not be using the DrivHIGH drivers!)
16. hit Finished,  then click Apply.

Enabling & Disabling Oversampling
---------------------------------
Simply run the registry file with the name fsaa-on to turn on Oversampling
& simply run the registry file named fsaa-off to turn it off.

Known Issues
------------
None at this time.

Known Bugs
----------
None at this time(Please report bugs & comments to obsidianknife@netzero.net)

Known Limitations
-----------------
None at this time.