[Japanese]
README.TXT                  MATROX GRAPHICS INC.                    2000.03.07

                     Matrox PowerDesk -- Windows NT 4.0


注意: このファイルには、まだ日本語に翻訳されていない最新情報が含まれている
場合もありますのでご了承ください。


目次
====

- このリリースについて
- インストール
- Matrox PowerDesk の使い方
- ハードウェア アクセラレーテッド 3D
- 注意、問題点および制限事項
- Matrox TV 出力
- [English...] DualHead notes [...English]


このリリースについて
====================

このリリースは、Matrox Windows NT ディスプレイ ドライバ です。x86
CPU で実行される Microsoft Windows NT、バージョン 4.0
(ビルド 1381 またはそれ以降のバージョン) でサポートされています。

この製品には、以下が含まれます。

- ディスプレイ ドライバ
- Matrox PowerDesk for Windows NT 4.0

[English...]

The display driver supports up to 16 graphics chips at a time. If one of
those chips has DualHead support, the display driver supports up to 17
displays at a time. (Note: A graphics card may have more than one graphics
chip. Also, the display driver must support each model of graphics card
installed in your computer.)

[...English]


インストール
============

Matrox PowerDesk をインストールするには、セットアップ プログラムを起動し、
その後は画面の指示に従います。

セットアップ プログラムで Matrox PowerDesk をインストールする場合、インスト
ール先のコンピュータで使用されている Matrox グラフィックスカード モデルがセ
ットアップ プログラムでサポートされていることが必要です。サポートされていな
い場合、ソフトウェアはインストールされません。

このソフトウェアを多数のシステムにインストールする場合、手順を部分的に自動化
するセットアップ オプションがあります。詳細については、このソフトウェアに含
まれている "setup_un.doc" ファイルを参照してください｡


Matrox PowerDeskの使用
======================

解像度の変更、モニターの選択、および Matrox PowerDesk の使用法については、
"online.doc"ファイルで説明されています。ワードパッドでこのファイルを表示でき
ます。


ハードウェア アクセラレータ 3D
==============================

3D ハードウェア アクセラレーションをサポートするために、Matrox Windows NT 4.0
ディスプレイ ドライバでは OpenGL インターフェイスが使用されています。
このインターフェイスには、MCD (Mini Client Driver) と ICD (Installable Client
Driver) の 2 つのタイプを使用できます。MCD では、Matrox Millennium、
Millennium II、Mystique、Mystique 220、および G100 ベースのグラフィックス
カードがサポートされます。ICD では、Matrox G200 ベース、G400 ベース、および
それ以上のグラフィックス カードがサポートされます。ICD は MCD よりも最適化に
適しています。

3D ハードウェア アクセラレーションには、次の制約があります。

- 現在、複数のカードを使用しているとき、アクセラレーションは使用できません。

- MCD は 8bpp (256色）モードおよび 24bpp (16777216 色）モードをサポートしま
  せん。16bpp (64,000 色)、および 32bpp (True Color) モードで、ハードウェア
  アクセラレーションが可能です。

- 使用できる解像度の制限は予想されています。すべての 3D モードで、ダブル
  バッファおよび/または Z バッファを扱うために余分なメモリが必要となり、
  このメモリは、表示には使用できません。


注意、問題点および制限事項
==========================

- PCI バスを 2 つ以上持つコンピュータ

  使用しているコンピューター カードをバス 0 以外の PCI バスにインストールす
  ると、フルスクリーンの [コマンドプロンプト] のスイッチかモード変更によっ
  て、ブルー スクリーン クラッシュが発生することがあります。この問題は現在
  調査中ですが、他の PCI スロットにカードを移動することで、問題を回避できる
  ことがあります。

  Windows NT で、PCI ブリッジを越えてインストールされたアダプターの競合をレ
  ポートするようなコンピューターがあります。この場合、Matrox Millennium ミニ
  ポートドライバは自身のカードにアクセスできません。システムが Millennium カ
  ードを見つけられない場合は、カードを他の PCI スロットに移動してみてくださ
  い。

  Microsoft Service Pack 3 (またはそれ以降のバージョン)for Windows NT 4.0
  をインストールすることにより これらの問題の多くが解決します。

- 仮想デスクトップを持つ DirectDraw

  一部の DirectDraw プログラムは、仮想デスクトップで正常に動作しません。
  通常のデスクトップで DirectDraw プログラムを実行するようお勧めします。

- 3D迷路 スクリーン セーバー

   "3D迷路" スクリーン セーバーの使用時、表示上の問題が生ずる場合があり
   ます。これは Microsoft Service Pack 2 for Windows NT 4.0 のインス
   トール後に起こる可能性があります。この表示の問題は Service Pack 3
   (またはそれ以降のバージョン)  で は解決されているようです。

- Winstone 97 の実行

  Winstone 97 ベンチマークを実行する際は、CenterPOPUP 機能（デフォルト
  設定）を必ず使用不能にしてください。CenterPOPUP 機能が使用可能になって
  いると、一部のテストでタイムアウト エラーが起きる場合があります。

- 複数のグラフィック カードを使用する場合の制限

  Windows NT 4.0 では、約 280 種類までの異なる表示モード（解像度、カラー
  パレット、およびリフレッシュ レートの組合せ）がサポートされます。
  Matrox グラフィック カードをコンピュータに複数インストールして使用して
  いる場合には、この上限を超えてしまう可能性もあります。

  コンピュータに Matrox カードが複数ある場合、Matrox "VESA 設定" オプ
  ション ボタンを選択すると、この Windows NT 4.0 の表示モード数上限を超
  える可能性がさらに高くなります。これは "VESA 設定" オプションが個々の
  解像度設定およびカラー パレット設定ごとに、異なる複数のリフレッシュ
  レートをサポートするためです。

  コンピュータに Matrox グラフィック カードが複数ある場合は、 "VESA
  設定" オプションを使わないことをお勧めします。Microsoft "画面のプ
  ロパティ" ダイアログ ボックスでリフレッシュ レートを変更すると
  "VESA 設定" オプションが有効になるので注意してください。

- 3D Studio MAX 1.2

  Matrox HEIDI ドライバの使用時、3D Studio Max 1.2 の動作に問題が生じた
  場合は、 "一般の設定" の "バス マスター の使用" チェック ボックス
  を無効にしてみてください。このチェック ボックスにアクセスするには、
  "スタート" ->  "プログラム" -> "Matrox PowerDesk NT" -> "Matrox
  表示プロパティ" -> "パフォーマンス" をクリックしてください。

- 3D Studio MAX 2.0

  3D Studio Max 2.0 の動作中に、HEIDI ソフトウェア エミュレーションと
  OpenGL アクセラレーションを相互に切り替えると、アニメーションの再生中
  ビューポートがちらつく原因となります。この問題は、3D Studio Max の動作
  中に表示設定（解像度またはカラー パレット）を変更した場合にも発生する
  可能性があります。この問題が起こったら、3D Studio Maxを終了して表示設定
  （解像度またはカラー パレット）を変更し、3D Studio MAXを再起動してみて
  ください。

[English...]

- 15-bit color palette support

  A 15-bit color palette is no longer supported.

- Multi-display desktop support

  With a multi-display desktop, all displays use the same color palette and
  display resolution. The maximum display resolution you can select is
  determined by the display with the highest maximum display resolution.

  If a display in your multi-display desktop doesn't support a selected
  display resolution, that display will automatically use a virtual display.
  With a "virtual display", parts of your "display area" are off-screen. You
  can move your mouse pointer to the edge of the screen to move the visible
  part of your virtual display. This virtual display feature is similar to
  using the Matrox zoom (PixelTOUCH) feature.

  Note: The "virtual display" feature isn't available with the secondary
  display of a DualHead-supporting graphics card. If a secondary display is
  part of your multi-display desktop, the maximum display resolution you can
  select is limited by the maximum display resolution of your secondary
  display. For more information on DualHead, see "DualHead notes".

  Software monitor settings help determine the maximum display resolution
  for each display. If software monitor settings aren't properly selected for
  all displays, one or more displays may become garbled or unusable if an
  unsupported display resolution is selected. For more information on
  selecting software monitor settings, see the online PowerDesk guide
  (online.doc).

- OpenGL support

  Note the following limitations related to the OpenGL driver included with
  Matrox PowerDesk:

    - OpenGL support may not be included in some versions of Matrox PowerDesk.
      For a version of Matrox PowerDesk with OpenGL support enabled, see
      the Matrox Web site (www.matrox.com/mga).

    - Under Windows NT 4.0, OpenGL acceleration isn't supported with
      Matrox MMS (Multi-Monitor Series) graphics cards or if you have more
      than one Matrox graphics card installed in your computer.

    - With DualHead-supporting graphics cards, OpenGL acceleration is
      available while using "DualHead Multi-Display" mode under
      Windows NT 4.0, (as long as there isn't another graphics card installed
      in your computer).

    - With the "Tribes" game, you may notice some minor display artifacts and
      the opening video introduction may not display properly.

    - Using 3D Studio Max 2.0, you may experience problems with the viewports
      being improperly redrawn. If this happens, simply click in a viewport
      to properly update their display. (This problem isn't present with
      version 2.5 or 3.0 of 3D Studio Max.)

    - To prevent display problems under Windows NT 4.0, the display driver
      may disable 3D screen savers while certain programs are running.

- System memory requirements

  Because of a limitation in Windows NT 4.0, you may experience problems
  if your computer doesn't have more system memory than the total amount
  of graphics memory used in your computer. To determine the amount of
  graphics memory used in your computer, add the total amount of graphics
  memory on each installed Matrox graphics card.

  Depending on your total amount of graphics memory, here are some
  recommended amounts of system memory for Windows NT 4.0:

      Graphics memory  |   System memory
          (total)      |   (recommended)
    -------------------+------------------
           32 MB       |   64 MB or more
           64 MB       |  128 MB or more
          128 MB       |  192 MB or more
          160 MB       |  256 MB or more

- Full-screen DOS support with multiple graphics chip

  If you have more than 10 graphics chips in your system (for example, 3
  Matrox MMS-Quad cards), your system may stop responding when running a
  DOS program in full-screen mode. If your DOS program supports it, run it
  in a DOS window.

[...English]


Matrox TV 出力
==============

Matrox グラフィック モードのモデルには、TV 出力をサポートするものがあります。
TV 出力をサポートしている場合、グラフィック カードに接続した TV またはビデオ
レコーダーにコンピュータ ディスプレイを表示または記録することができます。

推奨
----
- TV 出力を使用してゲームを行う場合は、640 ｘ 480 のディスプレイ解像度を使用
   することをお薦めします。これはTV の解像度能力がほとんどのコンピュータの
   モニターよりも低いためです｡さらに高いディスプレイ解像度（800 ｘ 600 または
   1024 x 768）を使用すると、TV ディスプレイはコンピュータのモニターのディス
   プレイほどシャープには見えない場合があります｡つまり、さらに細かいものは TV
   では表示できない場合があります。

- (Matrox G100/G200 カード用)
   Matrox のデフォルトのアドバンス TV 出力設定は、ほとんどの TV でほとんどの
   コンピュータ グラフィックス（たとえば、コンピュータ ゲームやWindows デスク
   トップ）を表示するのに向いています｡放送規格に基づいた、フル スクリーン ビ
   デオの表示にさらに適したアドバンス TV 出力設定があります。この設定は以下
   のとおりです。

  NTSC
     明るさ       : 180
     コントラスト : 234
     鮮やかさ     : 137
     色合い       : 0

  PAL
     明るさ       : 167
     コントラスト : 255
     鮮やかさ     : 138
     色合い       : 0

  注意: 理想的な設定にするには､TV の設定を調整することも必要かもしれません｡
  ほとんどの市販ビデオ装置のデフォルトの明るさ､コントラスト、鮮やかさ､色合い
  の設定は、放送規格より高いです。これらの設定は、ビデオを表示するのには通常
  OKですが、コンピュータ グラフィックスではOKでない場合があります。（これは、
  Matrox のデフォルトの TV 出力設定がビデオにとって理想的な設定より低いから
  です｡）TV の設定を調整する方法の詳細については、TVのマニュアルを参照して
  ください｡


詳細情報
--------
画面設定の詳細については、Matrox のマニュアルとオンライン マニュアルを参照し
てください｡使用しているゲームのディスプレイ解像度を変更する方法についての詳
細は、そのマニュアルを参照してください｡

注意: Matrox ズーム機能と仮想デスクトップ機能は TV 出力モードではサポートされ
ません。

また、使用しているコンピュータに複数の Matrox グラフィックス カードがインス
トールされている場合、TV 出力モードはサポートされません。

[English...]

Note: For TV output with full-screen DOS display modes under Windows NT 4.0,
only text display modes (02h, 03h) are supported.


DualHead notes
==============

Certain Matrox graphics cards can use one graphics chip to control two
separate displays -- this is the Matrox "DualHead" feature. If you have a
DualHead-supporting graphics card, note the following under Windows NT 4.0:

- DualHead software controls (on the Matrox PowerDesk "DualHead" property
  sheet) are only available if, when Windows NT 4.0 restarts, a secondary
  display is connected to your DualHead-supporting graphics card. For more
  information on DualHead software controls, see context-sensitive help.

- The "VESA settings" option isn't available when you're using a TV as your
  secondary display.

- With the "DualHead Multi-Display" feature, DirectDraw and OpenGL
  acceleration is available for the main and secondary displays of your
  DualHead-supporting graphics card.

- With the "DualHead Multi-Display" feature, all displays in your system
  may be limited by the display capabilities of the secondary display of
  your DualHead-supporting graphics card. Specifically:

  - Only a 16- or 32-bit color palette is available.

  - The Matrox zoom feature (PixelTOUTCH) is unavailable.

  - The mouse pointer is drawn entirely by the software. As a result, the
    mouse pointer may flicker or disappear while it's in an area of the
    display that's being redrawn quickly (for example, a video window).

  - Because the secondary display doesn't support the "virtual display"
    feature, the maximum display resolution of a multi-display desktop is
    limited by the maximum display resolution of the secondary display.

- With the "DualHead Zoom" feature, video (for example, DVD video) may 
  appear as a solid color on your secondary display. This limitation 
  occurs if the "DualHead Zoom" feature is used on a region that's using 
  hardware-based video overlay.

- The "DualHead Clone" feature is unavailable if your DualHead-supporting
  graphics card isn't controlling the primary display of your computer.
  The "primary display" of your computer is the one that first displays
  information when your computer restarts. For information on how to change
  which graphics card controls your primary display, see your system manual.

- With the "DualHead Clone" feature, both the main and secondary
  display of your DualHead-supporting graphics card use the same monitor
  settings (specifically, the same vertical refresh rate).

  If your secondary display is a TV, the vertical refresh rate is determined
  by the TV standard selected on the Matrox PowerDesk "Monitor" property
  sheet (60 Hz for NTSC, 50 Hz for PAL).

  If your secondary display is a computer monitor, the "Monitor" property
  sheet isn't available. In this case, use the "Refresh Frequency" control
  on the "Settings" property sheet to change your vertical refresh rate. If
  you select a refresh rate or display resolution that isn't supported by
  either display, one or both displays may become garbled or unusable.

- With the "DualHead Clone" feature, the virtual desktop feature is
  unavailable.

[...English]
