1. Before Using the Printer

1.1. Product series introduction

Product series parameters | M6700D series | M6700DW / M6760DW series | M7100DN series | M7100DW / M29DW series | M6800FDW / M6860FDW series | M7200FD series | M7200FDN series | M7200FDW /L2710FDW series
Interface type | USB | ● | ● | ● | ● | ● | ● | ● | ●
NET |  | ● | ● | ● | ● |  | ● | ●
Wi-Fi |  | ● |  | ● | ● |  |  | ●
Print Language | GDI | ● | ● |  |  | ● |  |  |
PDL |  |  | ● | ● |  | ● | ● | ●
Control Panel | LCD | ● | ● | ● | ● | ● | ● | ● | ●
Print Speed | A4 | 30ppm | ● | ● |  |  | ● |  |  |
33ppm |  |  | ● | ● |  | ● | ● | ●
Letter | 32ppm | ● | ● |  |  | ● |  |  |
35ppm |  |  | ● | ● |  | ● | ● | ●
Automatic Two-Sided Printing | ● | ● | ● | ● | ● | ● | ● | ●
NFC function |  | ● |  | ● | ● |  |  | ●
Mute printing | ● | ● | ● | ● | ● | ● | ● | ●
Copy | ● | ● | ● | ● | ● | ● | ● | ●
Scan | ● | ● | ● | ● | ● | ● | ● | ●
Fax |  |  |  |  | ● | ● | ● | ●
Scan to U-disk |  |  | ● | ● | ● | ● | ● | ●
ADF |  |  | ● | ● | ● | ● | ● | ●

(●: Support; Blank: Unsupport)

| Note: | • This product series is subject to additions or changes without prior notice. • For machine with the fax feature, it needs to execute language, system and fax settings following instructions on the panel in first startup or after restoring to factory settings. • For this user manual, the "ADF" is short for automatic document feeder.

1.2. Supplied Accessories

Name | Parts
Toner cartridge |
Drum component |
USB Interface Cable |
Power Cord |
CD |
Quick Setup Guide |
Pantum Warranty |

| Note: | • The Pantum Warranty may not be attached in some regions.

1.3. Product View

Side view

1 | Cover of automatic document feeder | This is used to remove the paper jammed in scanning for the ADF.
2 | Feed tray of automatic document feeder | This is used to place originals scanned from the ADF.
3 | Exit tray of automatic document feeder | Prevent originals scanned from falling off.
4 | Cover of scanner | Open the cover of scanner to place the scanned originals on its glass plate.
5 | Output Bin | For storing the printed paper.
6 | Front USB interface | This is used to scan to an U-disk without a computer.
7 | Control Panel | Indicate printer status to conduct set operation.
8 | NFC (Near Field Communication) label | Touch this label on mobile device to download or start Pantum printer App and connect Wi-Fi Directly.
9 | Glass Platen | This is used to place originals scanned from platen.
10 | Output Tray | To prevent the printed paper from falling.
11 | Front Cover | To open the front cover to take out the laser toner cartridge.
12 | Manual feed tray | For placing mediums that are printed in manual feed tray.
13 | Power switch | Turn the power on or off and press this button under Ready state to enter energy-saving mode. Press and hold this button for more than 2s to turn the printer power off.
14 | Automatic Feeder Tray | For placing mediums that are printed in auto feed tray.
15 | Paper deflector of manual feed tray | Slide paper deflector to adapt to paper width | 16 | Paper width deflector of auto feed tray | Slide paper width deflector to adapt to paper width. | 17 | Paper length deflector of auto feed tray | Slide paper length deflector to adapt to paper length. | 18 | Clip of extended tray of auto feed tray | For adjustment of length extension of the tray .

Rear View

1 | LINE interface (only for machine with the fax feature.) | Telephone line interface, used for connection of this product to the telephone circuit.
2 | EXT. interface (only for machine with the fax feature.) | Extension interface, used for connection with external extension telephone.
3 | USB Interface | For connecting product to computer with USB cable.
4 | Network Interface | For connecting product to network with network cable.
5 | Power Interface | For connecting product to power with power cord.
6 | Rear Cover | For paper release when it gets jammed.
7 | Duplex Printing Unit | For paper feed at duplex printing and paper release when paper gets jammed at duplex printing.

| Note: | Note: • Printer appearance may differ because of various models and functions, so the schematic diagram is only for your reference.

1.4. Laser Toner Cartridge

Laser toner cartridge is composed of drum component and toner cartridge.

Service life of drum component

Type | Average Print Volume
Standard drum component | About 12000 Pages(Based on ISO 19752 standard)
High volume drum component | About 25000 Pages(Based on A4/LTR size (3pages/job) )

Service life of toner cartridge

Type | Average Print Volume
Standard-volume toner cartridge | About 1500 Pages(Based on ISO 19752 standard)
High-volume toner cartridge | About 3000 Pages/6000 Pages(according to ISO 19752 standard)
Super large volume catridge | About 11000 Pages(Based on ISO 19752 standard)

| Note: | • The model is subject to increase without notice. • Consumables capacity may vary with different using types. • The Company does not recommend using consumables other than the original consumables provided, as any damages caused by non-original consumables are not covered by the scope of warranty. • Toner cartridge appearance may differ because of multiple volume and models, so the schematic diagram is only for your reference. • High volume drum component and super large volume catridge are only applicable to some models, please refer to the specifications of the model that you actually purchase.

1.5. Control Panel

1.5.1. Overview of control panel

The layout of the printer control panel is shown below:

Control panel without the fax feature

No. | Name | Functions
1 | LCD Display | Display operation interface and product information.
2 | Copy Button | Press this button to enter into copy mode.
3 | Scan Button | Press this button to enter into scan mode.
4 | ID Card Copy Button | Press this button to enter into ID Card Copy mode.
5 | Wi-Fi button | Short press Wi-Fi button to turn on direct Wi-Fi connection of the printer and automatically print out "Mobile Device Wi-Fi Connection Wizard" page (for models with Wi-Fi function only). Long press Wi-Fi button for over 2s to start WPS when Wi-Fi is not connected or to disconnect Wi-Fi when it has already been connected (for models with Wi-Fi function only). Open save toner function(applicable to non-Wi-Fi model only).
6 | Bill Copy Button | Press this button to enter into Bill Copy mode.
7 | Cancel | Execute cancel operation Idle state interface under copy mode, to reset the "Number of Copies" to 01.
8 | Start Button | This is used to start relevant operations after finishing operation settings. In case of a feed failure, please press this key for pick-up and printing again.
9 | Menu | Open the main menu of control panel
10 | Back | Return to the previous menu.
11 | OK | Confirm the selection on screen.
12 | UP | Scroll through the menus and options . Increase 1 copy on the ready interface of Copy mode.
13 | Down | Scroll through the menus and options . Decrease 1 copy on the ready interface of Copy mode.
14 | Status Light | Indicate the status of printer. (Please see Chapter 1.6).

Control panel with the fax feature

No. | Name | Functions
1 | LCD Display | Display operation interface and product information.
2 | Numeric keyboard | Dial or input letters, numbers or characters. (Please see Chapter 1.5.2).
3 | Fax | Press this button to enter into the Fax mode.
4 | Copy Button | Press this button to enter into copy mode.
5 | Scan Button | Press this button to enter into scan mode.
6 | Speaker | This is used to manually receive and send faxes under Fax mode, or for phone calls.
7 | ID Card Copy Button | Press this button to enter into ID Card Copy mode.
8 | Redial/Pause | This is used to redial the last number dialed before under Standby mode or to insert a pause symbol in the fax number under Edit mode.
9 | Bill Copy Button | Press this button to enter into Bill Copy mode.
10 | Wi-Fi button | Short press Wi-Fi button to turn on direct Wi-Fi connection of the printer and automatically print out "Mobile Device Wi-Fi Connection Wizard" page (for models with Wi-Fi function only). Long press Wi-Fi button for over 2s to start WPS when Wi-Fi is not connected or to disconnect Wi-Fi when it has already been connected (for models with Wi-Fi function only). Open save toner function(applicable to non-Wi-Fi model only).
11 | Contacts | This is used to enter quickly the Phone Book option under Fax mode.
12 | Cancel | Execute cancel operation Idle state interface under copy mode, to reset the "Number of Copies" to 01.
13 | Start Button | This is used to start relevant operations after finishing operation settings. In case of a feed failure, please press this key for pick-up and printing again.
14 | Menu | Open the main menu of control panel
15 | Back | Return to the previous menu.
16 | OK | Confirm the selection on screen.
17 | UP | Scroll through the menus and options . Increase 1 copy on the ready interface of Copy mode.
18 | Down | Scroll through the menus and options . Decrease 1 copy on the ready interface of Copy mode.
19 | Status Light | Indicate the status of printer. (Please see Chapter 1.6).

1.5.2. Function of numeric keyboard

Sometimes it needs to input names and numbers in executing some tasks. Letters, numbers and characters on the keyboard are distributed as below:

Keys | Numbers, letters and characters distributed
0 | 0
1 | @ / ; . 1
2 | a b c A B C 2
3 | d e f D E F 3
4 | g h I G H I 4
5 | j k l J K L 5
6 | m n o M N O 6
7 | p q r s P Q R S 7
8 | t u v T U V 8
9 | w x y z W X Y Z 9
* | （Space） & + , - * % ~ ! $ ( ) [ ]
# | # = ' | _ ? " : { } < >

| Note: | • It may not allow to input all special characters above mentioned in different input environments. a. Input of fax/phone number. It supports only inputting with 0-9 number keys and the "*" and "#" keys. In addition, it is available to input spaces with the Down key and the symbol "-" with the Redial/Pause key. b. Mixed input of letters, numbers and symbols. It is only allowed to input with 0-9 number keys and the "*" and "#" keys. Specific corresponding characters are different according to the difference of input environments. (Under this condition, pressing the Down key could make the cursor move backward; the symbol "-" could not be input with the Redial/Pause key.) • When inputting a number or name, short pressing Cancel could clear the last number or character; while to clear all numbers or characters, please long press it. You may also use the Up key to clear the last number or character.

1.6. Function of status indicator

The meanings of status displayed by the status indicator are as below:

No. | Status displayed by the status indicator | Status | Status Description
1 |  | Die out | Shutdown or sleep state
2 |  | Green indicator normally on | Printer is ready
3 |  | Green indicator blinks | Operative modes of Print, Copy, Scan, Fax and others
4 |  | Orange indicator blinks | Low toner warning
5 |  | Red indicator normally on | • Toner cartridge error (uninstalled ink cartridge, unmatching ink cartridge, invalid toner cartridge) • Drum unit error (the drum units are not installed, not compatible or come to the end of their service lives.) • Paper error (a paper out, paper jam or feed failure occurs) • Scan error (a scanning failure occurs, and the ADF has an open cover or a paper jam.) • Fax error or printer error such as the front cover of the printer is open.

1.7. Function of power indicator

No. | Status displayed by power indicator | Status | Status Description
1 |  | Die out | Shutdown status
2 |  | Always on | Booting and ready states
3 |  | Blink | Sleep mode