16. Product Specifications

| Note: | • Specification values vary slightly from printers with different models with different functions ,and product specifications vary from different countries and regions. • These values are based on the initial data. For more information about the latest specifications, please visit: www.pantum.com.

16.1. Overview of the Specifications

Product Size(W*D*H) | M6700 Series:415mm*365mm*310mm
M6800/M7100/M7200/M29/L2710 Series: 415mm*360mm*352mm
Product weight (exclusive of the random toner cartridge and packaging) | M6700 Series: 9.5Kg
M6800/M7100/M7200/M29/L2710 Series: 10Kg
Print Environment | Print temperature range:10-32 (5-35)℃
Print humidity range:20%RH~80%RH
Power Voltage | 110V Model: AC100~127V, 50Hz/60Hz,9A
220V Model: AC220~240V, 50Hz/60Hz,4.5A
Noise (acoustic pressure level) | Print/scan: ≤52dB(A)
Standby: ≤30dB(A)
Mute mode: ≤46 dB (A)
Enter network standby time: | 5 minutes
Power Consumption | Network standby: the model with wireless function: 2.366W the model without wireless function: 1.888W
Standby: ≤ 45W
Shutdown: ≤ 0.5W
TEC: conforming to requirements of EnergyStarV2.0 and Chinese energy efficency rating
Operating System | Microsoft Windows XP/ Windows Vista/ Windows 7/ Windows 8/ Windows 8.1/ Windows 10/ Windows Server 2003/ Windows Server 2008/ Windows Server 2012（32/64 Bit）
macOS 10.8/10.9/10.10/10.11/10.12/10.13/10.14
Linux (Ubuntu 14.04/ Ubuntu 16.04/ Ubuntu 18.04)
Versions higher than iOS 7.0
Android 4.4-9.0
Communication interface | Hi-speed USB 2.0
IEEE802.3 10Base-T/100Base-Tx
IEEE802.11b/g/n (support WPS)

16.2. Print Specifications

Print Speed | Please see Chapter 1.1.
Print Time of First Page | ≤8.5sec
Print Language | Please see Chapter 1.1.

16.3. Copy Specifications

Copy Speed | 30cpm(A4)/33cpm(Letter)
FCOT | Flatbed <10 seconds ADF <12 seconds
Maximum Pages for Successive Print | 99 pages
Zoom Ratio | 25%~400%
Other Copy Functions | "ID copy, Receipt copy, N-up copy, Clone copy"

16.4. Scan Specifications

Scan Type | Flatbed+ADF
Maximum Scan Size | Flatbed: 216×297mm ADF: 216×356 mm
Chromoscan | Yes
Scan Output Function | Scan to E-mail, PC, FTP and USB

16.5. Fax specification (applicable to machine with a fax)

Fax Type | Black-and-white
Modem Speed | 33.6Kbps
Fax Memory | 650 pages
Encoding | MH/MR/MMR/JBIG
Compatibility | ITU-T sg3/ECM
Other Fax Functions | PC-FAX (Send), Fax Filtering, Group Sending, Fax Forwarding, Speed Dial, Group Dial, Delay Sending, Auto Redial, Auto Receive, Auto Shrink, Mobile Fax
Environment | PSTN、PBX、VOIP

Company Name: Magnell Associate, Inc. ( DBA NEWEGG.COM ) Office address:17560 Rowland St. City of Industry, CA 91748 TEL: （626）271-9700 USA Only