Display Modes

The table that follows lists the various combinations of resolution, color-depth, and vertical refresh rate (in Hz) supported by your 3dfx Voodoo card in Windows 95, 98, or NT 4.0. The 640x480, 16 color VGA mode listed is only available as a Windows Desktop mode, and is not supported by Direct3D, Glide, or OpenGL. All of the other display modes listed are fully supported by the Voodoo card in Direct3D, Glide, and OpenGL.

Color-depth (in bits-per-pixel): | 4 bpp | 8 bpp | 16 bpp | 32 bpp
Number of Colors: | 16 (VGA) | 256 (SVGA) | 65K (High Color) | 16.7M (True Color)
Resolution:
640x480 | 60 | 60, 72, 75, 85, 100, 120, 140, 160
800x600 | - | 56, 60, 72, 75, 85, 100, 120, 140, 160
960x720 | - | 60, 75, 85
1024x768 | - | 60, 70, 75, 85, 100, 120
1152x864 | - | 60, 70, 75, 85, 100, 120
1280x960 | - | 60, 75, 85
1280x1024 | - | 60, 75, 85, 100
1600x1024 | - | 60, 76, 85, 100
1600x1200 | - | 60, 65, 70, 75, 80, 85, 100
1792x1344 | - | 60, 75
1856x1392 | - | 60, 75
1920x1080 | - | 60, 72, 75, 85
1920x1200 | - | 60, 76, 85
1920x1440 | - | 60, 75
2048x1536 | - | 60, 75